CUT SHEET DCP-1 and DCP-2



 DCP-1

SmartGuard 1 Gang duplex receptacle cover – mounting screw not included

Part 1 Gang Device Cover

Dimension 2.19 x 4.1 x .33

Application Screws into device

Installation Method Installs with 1 screw over device

Removal Method Unscrew and remove

Mil/Thickness 60 mil

Item Weight .3 oz.



DCP-2

SmartGuard 2 Gang duplex receptacle cover – mounting screws not included

Part 2 Gang Device Cover

Dimension 3.7 x 4.18 x .33

Application Screws into device

Installation Method installs with 2 screws over device

Removal Method Unscrew and remove

Mil/Thickness 60 mil

Item Weight .5 oz.

**UL 514C – SmartGuard Covers Meet Standards for Fire Rating and Dielectric Strength**